(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "Zorro3" (in_bom yes) (on_board yes)
    (property "Reference" "CN" (id 0) (at 1.27 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Zorro3" (id 1) (at 12.7 -69.85 90)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Zorro3_0_1"
      (rectangle (start 0 0) (end 25.4 -129.54)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "Zorro3_1_1"
      (pin power_out line (at -2.54 -2.54 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -12.7 180) (length 2.54)
        (name "+12" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -127 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "100" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -15.24 0) (length 2.54)
        (name "~{CFGOUT}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -15.24 180) (length 2.54)
        (name "~{CFGIN}" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -17.78 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -17.78 180) (length 2.54)
        (name "~{C3}" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -20.32 0) (length 2.54)
        (name "CDAC" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -20.32 180) (length 2.54)
        (name "~{C1}" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -22.86 0) (length 2.54)
        (name "~{CINH}" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -22.86 180) (length 2.54)
        (name "~{MTCR}" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -25.4 0) (length 2.54)
        (name "~{INT2}" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -2.54 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -25.4 180) (length 2.54)
        (name "-12" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -27.94 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -27.94 180) (length 2.54)
        (name "~{INT6}" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -30.48 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -30.48 180) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -33.02 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -33.02 180) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -35.56 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -35.56 180) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -38.1 0) (length 2.54)
        (name "~{LOCK}" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -5.08 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -38.1 180) (length 2.54)
        (name "A8/D0" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -40.64 0) (length 2.54)
        (name "FC0" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -40.64 180) (length 2.54)
        (name "A9/D1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -43.18 0) (length 2.54)
        (name "FC1" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -43.18 180) (length 2.54)
        (name "A10/D2" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -45.72 0) (length 2.54)
        (name "FC2" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -45.72 180) (length 2.54)
        (name "A11/D3" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -48.26 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -48.26 180) (length 2.54)
        (name "A12/D4" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -50.8 0) (length 2.54)
        (name "A13/D5" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -5.08 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 27.94 -50.8 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -53.34 0) (length 2.54)
        (name "A14/D6" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 27.94 -53.34 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -55.88 0) (length 2.54)
        (name "A15/D7" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 27.94 -55.88 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -58.42 0) (length 2.54)
        (name "A16/D8" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -58.42 180) (length 2.54)
        (name "~{BERR}" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -60.96 0) (length 2.54)
        (name "A17/D9" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -60.96 180) (length 2.54)
        (name "~{MTACK}" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -63.5 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -7.62 0) (length 2.54)
        (name "+5" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -63.5 180) (length 2.54)
        (name "E" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -66.04 0) (length 2.54)
        (name "~{DS0}" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -66.04 180) (length 2.54)
        (name "A18/D10" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -68.58 0) (length 2.54)
        (name "~{RST}" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -68.58 180) (length 2.54)
        (name "A19/D11" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -71.12 0) (length 2.54)
        (name "~{HALT}" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -71.12 180) (length 2.54)
        (name "A20/D12" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -73.66 0) (length 2.54)
        (name "A22/D14" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -73.66 180) (length 2.54)
        (name "A21/D13" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -76.2 0) (length 2.54)
        (name "A23/D15" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -7.62 180) (length 2.54)
        (name "+5" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -76.2 180) (length 2.54)
        (name "~{BR}" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -78.74 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -78.74 180) (length 2.54)
        (name "~{BGACK}" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -81.28 0) (length 2.54)
        (name "A31/D31" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -81.28 180) (length 2.54)
        (name "~{BG}" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -83.82 0) (length 2.54)
        (name "A30/D30" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 27.94 -83.82 180) (length 2.54)
        (name "~{DTACK}" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -86.36 0) (length 2.54)
        (name "A29/D29" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -86.36 180) (length 2.54)
        (name "READ" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -88.9 0) (length 2.54)
        (name "A28/D28" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -10.16 0) (length 2.54)
        (name "~{OWN}" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -88.9 180) (length 2.54)
        (name "~{DS2}" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -91.44 0) (length 2.54)
        (name "A27/D27" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -91.44 180) (length 2.54)
        (name "~{DS3}" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -93.98 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -93.98 180) (length 2.54)
        (name "~{CCS}" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -96.52 0) (length 2.54)
        (name "SD0/D16" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -96.52 180) (length 2.54)
        (name "A26/D26" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -99.06 0) (length 2.54)
        (name "SD1/D17" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -99.06 180) (length 2.54)
        (name "A25/D25" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -101.6 0) (length 2.54)
        (name "SD2/D18" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -10.16 180) (length 2.54)
        (name "-5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -101.6 180) (length 2.54)
        (name "A24/D24" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -104.14 0) (length 2.54)
        (name "SD3/D19" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -104.14 180) (length 2.54)
        (name "SD7/D23" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -106.68 0) (length 2.54)
        (name "SD4/D20" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -106.68 180) (length 2.54)
        (name "SD6/D22" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -109.22 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -109.22 180) (length 2.54)
        (name "SD5/D21" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -111.76 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "87" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -111.76 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "88" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -114.3 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "89" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -2.54 -12.7 0) (length 2.54)
        (name "~{SLAVE}" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at 27.94 -114.3 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "90" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -116.84 0) (length 2.54)
        (name "SENSEZ3" (effects (font (size 1.27 1.27))))
        (number "91" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -116.84 180) (length 2.54)
        (name "7Mhz" (effects (font (size 1.27 1.27))))
        (number "92" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -119.38 0) (length 2.54)
        (name "DOE" (effects (font (size 1.27 1.27))))
        (number "93" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -119.38 180) (length 2.54)
        (name "~{IORST}" (effects (font (size 1.27 1.27))))
        (number "94" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -121.92 0) (length 2.54)
        (name "~{BCLR}" (effects (font (size 1.27 1.27))))
        (number "95" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect non_logic (at 27.94 -121.92 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "96" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -2.54 -124.46 0) (length 2.54)
        (name "~{FCS}" (effects (font (size 1.27 1.27))))
        (number "97" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 27.94 -124.46 180) (length 2.54)
        (name "~{DS1}" (effects (font (size 1.27 1.27))))
        (number "98" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -2.54 -127 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "99" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
